85726425101670
0_amslib2_kc5
1x2Jumper


0
2
2
0_amslib2_kc5
1x4_0.1in_Header


0
4
4
0_amslib2_kc5
1x4_0.1in_Header_nob


0
4
4
0_amslib2_kc5
1x8_0.1in_Header


0
8
8
0_amslib2_kc5
1x8_0.1in_Header_2mm_nob


0
8
8
0_amslib2_kc5
1x8_0.1in_Header_nob


0
8
8
0_amslib2_kc5
5VRelay_Z3811-ND


0
4
4
0_amslib2_kc5
495-2470-1-ND_1uFFilm
C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf
C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor
0
2
2
0_amslib2_kc5
495-2470-1-ND_FilmCap


0
2
2
0_amslib2_kc5
0805_handsolder_noref
Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
capacitor handsolder
0
2
2
0_amslib2_kc5
1206_handsolder_noref
Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
0_amslib2_kc5
AD629_8SOIC
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)
SOIC 1.27
0
8
8
0_amslib2_kc5
AD7940_8MSOP
8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
8
8
0_amslib2_kc5
AD7940_14bitadc_SOT23-6


0
6
6
0_amslib2_kc5
AD8422_8MSOP
8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
8
8
0_amslib2_kc5
AD8422_8SOIC
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)
SOIC 1.27
0
8
8
0_amslib2_kc5
AD8479_8SOIC
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)
SOIC 1.27
0
8
8
0_amslib2_kc5
ADS7835_8VSSOP


0
8
8
0_amslib2_kc5
AXICOM_P2_Relay_V23079


0
10
10
0_amslib2_kc5
Arduino_Nano
Through hole straight pin header, 1x15, 2.54mm pitch, single row
Through hole pin header THT 1x15 2.54mm single row
0
30
30
0_amslib2_kc5
BarrelJack_839-1516-ND
Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf
Power Jack
0
3
3
0_amslib2_kc5
Bourne_Trimmer_TC33


0
3
3
0_amslib2_kc5
Button_Tact_TEConn_450-1792-1-ND


0
4
4
0_amslib2_kc5
CUI_DCWN03A-15


0
8
8
0_amslib2_kc5
DBPW06F-12


0
7
7
0_amslib2_kc5
EasyDriver


0
17
17
0_amslib2_kc5
FilmCap_495_2470_1_ND


0
2
2
0_amslib2_kc5
IF_D91


0
4
2
0_amslib2_kc5
IF_D98


0
6
4
0_amslib2_kc5
IF_D98_v2


0
6
4
0_amslib2_kc5
IF_E98


0
6
4
0_amslib2_kc5
IF_E98_v2


0
6
4
0_amslib2_kc5
INA149_8SOIC
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)
SOIC 1.27
0
8
8
0_amslib2_kc5
LD1117V33_TO220AB
TO-220-3, Vertical, RM 2.54mm
TO-220-3 Vertical RM 2.54mm
0
3
3
0_amslib2_kc5
LOGO


0
0
0
0_amslib2_kc5
LQFP-64_10x10mm_Pitch0.5mm_widetrace
64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)
QFP 0.5
0
64
64
0_amslib2_kc5
LV7805CV_TO220AB
TO-220-3, Vertical, RM 2.54mm
TO-220-3 Vertical RM 2.54mm
0
3
3
0_amslib2_kc5
MIDAS_2LLCD


0
16
16
0_amslib2_kc5
MIDAS_20x4LCD_MC42005A6W


0
16
16
0_amslib2_kc5
MolexBNC


0
2
2
0_amslib2_kc5
PJ-102A


0
3
3
0_amslib2_kc5
PTV09A_Top


0
3
3
0_amslib2_kc5
Phoenix_5mm_screwterminal
Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm^2 drill 1.3mm pad 2.6mm
0
2
2
0_amslib2_kc5
Reg_m5V_MC79L05ACLPR
TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
0_amslib2_kc5
SN74ACT08_SOIC-14
SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
14
0_amslib2_kc5
SOT-23-5-HandSolder
5-pin SOT23 package
SOT-23-5 hand-soldering
0
5
5
0_amslib2_kc5
SOT23-6


0
6
6
0_amslib2_kc5
SOT223-3LD-PL-1


0
4
4
0_amslib2_kc5
Switch_3termSL_4.7mmx2mmx0.76mm


0
3
3
0_amslib2_kc5
TO-92_Inline_Narrow_Oval
TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)
to-92 sc-43 sc-43a sot54 PA33 transistor
0
3
3
0_amslib2_kc5
TO-220-3_Vertical
TO-220-3, Vertical, RM 2.54mm
TO-220-3 Vertical RM 2.54mm
0
3
3
0_amslib2_kc5
Testpad


0
1
1
0_amslib2_kc5
URA2409YMD-10WR3


0
6
6
0_amslib2_kc5
XP_IZ1215S


0
7
7
